



* Open the updater on your Windows computer
* Connect NGC HDMI to a Windows computer via a USB cable
* Once properly connected, the BitFunx logo will turn colorful and the bottom left corner will show that the device is connected



* Click the drop-down box icon, select the latest firmware, and then click Update and wait for the update to complete
* 
* 